BusinessPhone Communication Platform 5.1
Commands > Commands 4000...4999

## 4316
Silent detect time VMU-HD

The detection of silence is implemented on the VMU-HD board. When silence is detected during recording of a voice message the central software will be informed and can take appropriate action.

This command defines the silence detection time. For detection, the state of silence must last for a certain period of time.

Valid values are 0, 5-30 seconds.

Default value is 10 seconds and 0 means no detection active.

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: PD1 © Ericsson Enterprise 2003