BusinessPhone Communication Platform 5.1
Commands > Commands 1000...1999

## 1910
Interface type

This command is used to specify the type of Basic Access connection mode. At connection to S-interface user mode is valid. At connection to T-interface network mode is valid. At connection to Q-interface network mode (Q-reference point) is valid.

Note

The selected type of connection has to correspond to DIP switching of interface type on BTU-B board.

Value = USER (-S) NETWORK (-T) NETWORK (-Q)

Default value NETWORK (-T)

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: PD1 © Ericsson Enterprise 2003