BusinessPhone Communication Platform 5.1
Commands > Commands 2000...2999

## 2109
MFE time 2

States the supervision time 2 during MFE signalling.

Supervises the reception of an MFE-signal if the other party is supposed to send an information signal. This time applies for the signals not handled by the command 2108 MFE time 1, MFE TIME 1.

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2003