BusinessPhone Communication Platform 5.1
Commands > Commands 1000...1999

## 1407
Maximum hold time

The command is used to determine the maximum time a call can be put on hold before it is released. Value 0-255 seconds.

This time supervision will be active when a call lacks a destination, e.g. when there is neither an answering position nor a rerouting position. Timeout results in disconnection of the external line in order to pre-vent “locking” it.

Note

When the call is in the ringing state, it can be supervised by means of command 1406 Wait time before ring back/rerouting at not answered calls.

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: PD1 © Ericsson Enterprise 2003