BusinessPhone Communication Platform 5.1
Warning Messages ASB 150 02 >

## 0x4C
RP Serial Communication Error

Default definition: |  | ERROR |
Used by block: |  | RP |
Category: |  | MAINTENANCE |

A transmit or receive error has been detected by a RP.

- D1: 0
- D2: Type of error

- Bit 0: Missing a part of a message
- Bit 1: Too long message received
- Bit 2: Error in the ML in a buffer for the transmission of an info message.
- Bit 3: Unexpected events in state
- Bit 4: Undefined DFD
- Bit 5: Receive error during transmit e.g. receive fault when waiting for ACK/NAK.
- Bit 6: 0
- Bit 7: 0

- D3: Undefined
- D4: Undefined

Revision: PH2 © Ericsson Enterprise 2003