BusinessPhone Communication Platform 5.1
Warning Messages ASB 150 02 >

## 0xE5
RP IPU Error

Default definition: |  | ERROR |
Used by block: |  | IPU |
Category: |  | DESIGNER |

Highest IPU warning level.

An extremely severe fault has been detected by the IPU software. There is no way of continuing the normal flow of control, so an immediate restart of the IPU board is required.

- D1: Originating IPU software block, high byte
- D2: Originating IPU software block, low byte
- D3: Details on the fault reason, high byte
- D4: Details on the fault reason, low byte

Revision: PH2 © Ericsson Enterprise 2003