BusinessPhone Communication Platform 5.1
Dialogs

## Destination Number Cross Reference Table

If the PABX has got several route connections to networks with different number plans, you can define up to four destination numbers, including predigits and destination group numbers.

To access the dialog, open the “Facilities” menu in the Configuration directory tree. Then open the “Least Cost Routing” submenu and click on “Destination Number Cross Reference Table”.

For more information about how to define an individual mailbox, see facility description Least Cost Routing (321/15534-ASB 150 02 Uen) and command 2250 Destination Number Cross Reference Table.

### Predigits

Enter the predigits that are defined for the trunk connection in the current direction.

### Destination Number

Enter the leading digits (up to 16) of a destination number. This number is required to identify the call costs.

### Destination Number Group

The number of the group. It is recommended to assign a number to each group. The number should be based on the official carrier prices.

The number series for list prices should always be ascending, starting with 0. For special prices (i.e. for tie lines), it is recommended to use a descending number series, starting with the highest number, which is 249. This way, it will be easier to maintain the information.

#### Actions

Submit |  | To set the changed parameters. |
Reload |  | To reload the current parameters. |

Revision: B © Ericsson Enterprise 2003