BusinessPhone Communication Platform 5.1
Commands > Commands 9000...9999

## 9111
NPI for private/public called number 1

The command is used to define the Number Plan Identifier (Number Plan and Type Of Number) of the called number.

Following combinations of NP’s and TON’s are available for the CN calls:

NP/TON | E.164 (ISDN)
| International, PUB/INT
| National, PUB/NAT
| Subscriber, PUB/SUBS
| Unknown, PUB/UNKN

NP/TON | PRIVATE NP (QSIG)
| Regional level 1, PNP/RL1 (regional)
| Regional level 0, PNP/RL0 (local)
| Unknown, PNP/UNK

NP/TON | UNKNOWN NP (QSIG)
| Unknown, UNK/UNK

Value:

PUB/INT

PUB/NAT

PUB/SUBS

PUB/UNK

PNP/UNK

PNP/RL0

PNP/RL1

UNK/UNK

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: PD1 © Ericsson Enterprise 2003