BusinessPhone Communication Platform 5.1
Dialogs

## Automatic Redial

With this feature, an extension can start the automatic redial of the last dialed external number. The automatic redial request is controlled by a programmable function key.

To access the dialog, open the “System” menu in the Configuration directory tree. Then open the “System facilities” submenu, and click on “Automatic Redial”.

In this dialog, you can set the following parameters:

2271 |  | Number of auto redial requests

2272 |  | Trunks available for auto redial

2273 |  | Auto redial trunk access retries

2274 |  | Auto redial answer supervision time

Furthermore, you can define the number of redial attempts and the time intervals (in seconds) when an automatic redial call is performed. A maximum of 10 entries are possible.

#### Actions

Submit |  | To send the settings to the system. |
Reload |  | To load the current system settings and to discard all entered data or changes. |

See facility description Last external Number redial (320/15534-ASB 150 02 Uen).

Revision: B © Ericsson Enterprise 2003