BusinessPhone Communication Platform 5.1
Signal Types, Internal Messages and CSW-Blocks > Internal Messages - Info Codes > Sorted by Info code

## 36 CTIFUNC

00h MONVERRQ |  | Query a monitor on an extension |
01h MONVERRSP |  | Positive acknowledge for query |
02h MONSTRTRQ |  | Start a monitor on an extension |
03h MONSTRTRSP |  | Response for start request |
04h MONSTRTACD |  | ACD response for start |
05h MONSTOPRQ |  | Stop a monitor on an extension |
06h MONSTOPRSP |  | Response for stop request |
07h MONSTOPACD |  | ACD response for stop request |
08h MONEND |  | Report a monitor end on an extension |
09h MONSUPPORT |  | Report if monitoring is supported at all |
10h ROUTETIMEOUT |  | Waiting timeout value for reroute destination |
11h CTKEYCODE |  | Keycode message from CT-block |
20h EVSTATUPD |  | Report device state update event |
21h EVDIRNUMCH |  | Report directory number change |
23h EVNAMEUPD |  | Report opposite / divertee name |
24h EVFORWARDUPD |  | Report update of call forwarding |
25h EVACDUPD |  | Report update of ACD-status |
26h EVFEATURE |  | Report activated features |
27h EVREPCALLREC |  | Report call record |
28h EVSLAVEUPD |  | Report slave state update event |
29h EVOPIDATA |  | Report special OPI data |
2Ah EVOPIQUE |  | Report status of OP queue |
2Bh EVINFOUPD |  | Report update of Info status |
2Ch EVFACUPD |  | Report update of facility status |
2Dh EVACDQUPD |  | Report ACD queue state update |
70h REQMAKECALL |  | Request to start a fresh call |
71h RSPMAKECALL |  | Response to a requested make call |
72h REQFWDSTAT |  | Request to report call forwarding info |
73h REQACDSTAT |  | Request to report ACD agent status |
74h REQCONFCALL |  | Request to start a conference |
75h RSPCONFCALL |  | Response to a requested conference |
76h REQFWME |  | Request a Follow Me on extension |
77h REQPICKUPIND |  | Request to do individual pickup |
78h RSPPICKUPIND |  | Response to a requested individual pickup |
79h REQINFO |  | Request an info on extension |
7Ah REQMESS |  | Request a message on extension |
7Bh REQDND |  | Request Do not disturb |
7Ch RSPDND |  | Response to a requested Do not disturb |
7Dh REQPCROUT |  | Request reporting of incoming calls |
7Eh RSPPCROUT |  | Response to a request PC controlled routing |
7Fh REQNEWDEST |  | Request reroute to new destination |
80h RSPNEWDEST |  | Response to a request new destination |
81h REQTRANSFER |  | Request transfer of a call |
82h RSPTRANSFER |  | Response to a requested transfer |
83h REQFORWARD |  | Request to initiate call forward |
84h RSPFORWARD |  | Response to a requested call forward |
85h REQANSWER |  | Request to answer a call |
86h REQCAMPON |  | Request to do a camp on |
87h REQPICKUPGRP |  | Request to pickup call from group |
88h RSPPICKUPGRP |  | Response to a request group pickup |
89h REQSNAPDEV |  | Request snapshot device |
8Ah RSPSNAPDEV |  | Response to a request snapshot device |
8Bh REQCB |  | Request to initiate call back |
8Ch REQBI |  | Request to initiate break in |
8Dh REQHOLD |  | Request to put a call on hold |
8Eh REQSNAPACD |  | Request snapshot ACD |
8Fh RSPSNAPACD |  | Response snapshot ACD |
90h REQDEFLECTCALL |  | Request deflection of an incoming call |
91h RSPDEFLECTCALL |  | Response deflection of an incoming call |
92h REQINFOSTAT |  | Request Info states/Info texts |
93h RSPINFOTXT |  | Response Info texts |
94h REQVOICEPG |  | Request a voice paging action |
95h RSPVOICEPG |  | Response to voice page command |
96h REQKEYLAYOUT |  | Request instrument key programming layout |
97h RSPKEYLAYOUT |  | Response instrument key programming layout |
98h REQOPIFUNC |  | Request special function of operator instrument |
99h REQSETTINGS |  | Request change of device settings |
9Ah RSPSETTINGS |  | Response to change of device settings |
9Bh REQLINKPOS |  | Request linking position |
9Ch RSPLINKPOS |  | Response linking position |

Revision: PD2 © Ericsson Enterprise 2003