BusinessPhone Communication Platform 5.1
Commands > Commands 1000...1999

## 1302
Outgoing digit transmission

The command states how the digits are sent from the interworking exchange. The initial value depends on the type of the BTU.

Type of BTU: |  | Value: |
BTU-A |  | 0 |
BTU-C |  | 0 |
BTU-E |  | 0 |
BTU-D |  | 2 |

0 = Decadic impulsing |  |

1 = DTMF |  |

2 = MFC |  |

3 = No sending of digits |  |

4 = MFE1 (2/5) |  |

5 = MFE2 (2/6) |  |

Value = 0-5

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: PD1 © Ericsson Enterprise 2003