BusinessPhone Communication Platform 5.1
Dialogs

## Trunk Routes

The facility creation dialog is used to create and delete facilities, change their directory numbers and names and select a facility for parameter editing.

To access the dialog, open the “Trunks” menu in the Configuration directory tree and click on “Trunk Routes”.

The following commands are available:

5401 |  | Create Trunk Route

5608 |  | Alter route number

6501 |  | Directory name

5501 |  | Delete trunk route

### Creating a facility

To create a new trunk route, enter the directory number in the “Directory Number” field in the “Create Trunk Route” section and click on the Create button.

If you have changed any directory numbers or directory names you will be asked whether you want to discard your changes. If you want to save your changes first, click on Cancel and press the Submit button before creating the new group.

### Changing a directory number and/or directory name

To change a Directory Number or Name, edit the numbers or names displayed in the Edit/Change Trunk Routes section and click on the Submit button.

### Editing the trunk parameters

To view and edit the Trunk Parameters, click on the Parameters link of the desired facility. If a directory number or name has been changed, you will be asked whether you want do discard these changes. To save your changes, choose Cancel and submit your changes before you click on the Parameters link.

### Deleting a trunk

To delete a facility, click on the facility’s Delete link. BMS will display a delete dialog.

Note

The first route can not be deleted!

See Facility Descriptions:

- Route Selection (444/15534-ASB 150 02 Uen).
- Trunk (486/15534-ASB 150 02 Uen).

Revision: B © Ericsson Enterprise 2003