BusinessPhone Communication Platform 5.1
Commands > Commands 6000...6999

## 6304
Bar outgoing calls?

In certain cases, e.g. when external/peripheral equipment for storage of call data is out of order, the desired logging is not possible. Using this command it is possible to select whether to permit subsequent outgoing external calls without logging or to restrict such calls until logging is again possible.

Note that it is always possible for the operator to initiate outgoing external calls irrespective of the value of this command.

Valid Values: YES / NO

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: D © Ericsson Enterprise 2003