BusinessPhone Communication Platform 5.1
Facilities

## Camp On – Inquiry

## Definition

An extension who, on inquiry, encounters busy tone, can camp the latest individually parked party on to the busy extension, via a transfer request.

## Use

Allows an OPERATOR equipped with an EXECUTIVE telephone or other extension to extend calls even if the called party is busy. This enables the extending party to go free and answer new calls.

## Operation

### ECONOMY-, STANDARD- and EXECUTIVE telephones

An extension connected to an external party initiates inquiry to an internal party.

If the inquirer receives busy tone, the external call can be camped on to the busy extension as follows:

1. Press Transfer.

- Lamps for both parked and called parties extinguish. The display shows idle information provided no other calls are parked.

The camped on party receives music on hold or silence.

See also facility description Call Waiting Indication (145/155 34-ASB 150 02 Uen).

The party who receives the camp on hears a short ring burst (analogue telephone two short tone bursts in handset).

If camp on is forbidden, depression of the Transfer‑key will be ignored.

### BASIC- and ANALOGUE telephones

An extension connected to an internal party initiates inquiry to another internal party.

If the caller receives busy tone, the external call can be camped on to the busy extension as follows:

1. By replacing handset, whereupon caller's telephone is free.

- Camped on party receives music on hold or silence.

See also facility description Call Waiting Indication (145/155 34-ASB 150 02 Uen).

If camp on is forbidden, the external party will recall the transferring extension.

### Recall

If a camped on external call remains unanswered after a programmable time, the transferring party will be recalled.

Note

Camped on internal calls do not lead to recall.

See also facility description Recall (440/155 34-ASB 150 02 Uen).

## Capacity

The number of external calls that can be camped on to an extension is unlimited.

## Limitations

Camp on cannot be undertaken if:

- The parties belong to different traffic groups that may not be interconnected
- The busy extension has a category that forbids camp on
- The extension has a facility category that forbids transfer before answer and camp on

## Programming

0108 |  | Camp-on allowed ?

An extension can be programmed individually to prevent camp on to the extension.

Default data: Yes, camp on allowed

## Equipment

None

Revision: B © Ericsson Enterprise 2003