BusinessPhone Communication Platform 5.1
Commands > Commands 6000...6999

## 6406
Automatic I/O activation

The command is used to determine the time for automatic activation of output on a fault-marked external communication channel. Timeout results in the fact that at the next output occasion a new attempt will be made to again use this communication channel.

Value = 0-11 min

If the time is set = 0, there will be no automatic activation attempt. A manual attempt can be made to start communication on a fault-marked communication channel by first setting the channel to passive and thereafter setting it to active again, see command 6402 Activate I/O ports?. This procedure includes the risk that data might be lost.

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: D © Ericsson Enterprise 2003