BusinessPhone Communication Platform 5.1
Warning Messages ASB 150 02 >

## 0x14
OS Internal Error

Default definition: |  | ERROR |
Used by block: |  | OS |
Category: |  | DESIGNER |

This code is used by OS to signal internal errors such as pointer errors, counter errors, etc.

- D1:
- D2: Sequence number

- 80H-8Fh: From file OSHWI*
- 90H-9Fh: From file OSTIM*

- D3: Undefined
- D4: Undefined

Revision: PH2 © Ericsson Enterprise 2003