BusinessPhone Communication Platform 5.1
Commands > Commands 4000...4999

## 4012
Sending a ready tone after announcement

The command defines whether a toneburst (TONE.OKAY) shall be sent to the operator after sending of the individual operator announcement has been completed.

Alternatives:

YES = A tone burst will be sent to the respective operator after the individual operator announcement has been send. |  |

NO = No tone burst will be sent to the respective operator after the individual operator announcement has been sent. |  |

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: PD1 © Ericsson Enterprise 2003