BusinessPhone Communication Platform 5.1
Commands > Commands 5000...5999

## 5211
Recall number

This command determines what digits are to form the recall number. Digits for trunk or route selection are to be included in the number specified.

Recall is a procedure in which an incoming call is not given direct access to the system. Instead, the call is terminated, after which the PABX makes an outgoing call to a predetermined number. This number is optional and should represent a party which is authorized for system access.

The number may contain the following characters:

0-9,*,# |  | Digit to be sent

- |  | Await second dial tone

Commands 5208 Recall control-5211 Recall number concern the recall function.

Valid values: 20 digits

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: C © Ericsson Enterprise 2003