BusinessPhone Communication Platform 5.1
Commands > Commands 1000...1999

## 1943
UU-information in ALERT message

This command states whether or not it is allowed to include UUI (User-to-User Information) in the ALERTING message at this interface.

Valid data:

No: not allowed |  |

Yes: allowed |  |

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: PD1 © Ericsson Enterprise 2003