BusinessPhone Communication Platform 5.1
Commands > Commands 8000...8999

## 8901
CTI port

This command can be used to define the port number and the individual number of the CTI port, where data transfer should be handled. The first two digits specify the board number, where the CTI port is located, the next three digits specify the individual number of the CTI port on the board.

##### Valid values: ppiii

- pp = Board position
- iii = Individual of a V24 (IO Unit) port

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: PD1 © Ericsson Enterprise 2003