BusinessPhone Communication Platform 5.1
Warning Messages ASB 150 02 >

## 0x97
Card Supervision Failure

Default definition: |  | STOP |
Used by block: |  | OM |
Category: |  | MAINTENANCE |

The supervision facility has detected an error. If the error was ‘no response from some card’, the attempt to communicate with the card in question is repeated five times, before the warning is sent.

- D1: 0
- D2: Card position
- D3: Undefined
- D4: Undefined

Revision: PH2 © Ericsson Enterprise 2003