BusinessPhone Communication Platform 5.1
Commands > Commands 0000...0999

## 0111
Diversion on busy at internal calls ?

The command defines if a diversion on busy in case of an internal call should be done. If the extension is a master and member of a tandem configuration the command data shall be copied to the slave and blocked for the slave's further use.

##### Valid data: Yes / No (default)

Minimum required authority level from telephone: 0

Accessible via BMS: Yes

Revision: PD6 © Ericsson Enterprise 2003