BusinessPhone Communication Platform 5.1
Commands > Commands 2000...2999

## 2056
Shut down reroute position

The command determines the shutdown reroute position. If the call terminator is in shutdown state the call will be rerouted to this shutdown reroute position. The shutdown reroute position is stated by its directory number.

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2003