BusinessPhone Communication Platform 5.1
Commands > Commands 0000...0999

## 0147
Type of meter info

Select type of metering information to be displayed.

During EXTERNAL calls it is possible to display different types of metering information, such as “Money”, “Pulses”, “Duration” etc. For incoming external calls “Duration” is always selected unless the function is disabled.

The information is displayed either when a menu key is pressed or automatically. “Automatically” means that the selected type of metering information is displayed without first pressing a menu key, and that the metering information is automatically updated during the call. If the function is disabled when the call is initiated, it can be temporarily enabled by pressing a menu key, see command 0148 Automatic display of metering info? for more details.

If selected metering information is not available, nearest “lower” information is displayed.

Example: If value 3 is programmed but the cost in local currency is not available, the number of metering pulses is displayed instead.

#####

0 |  | display nothing (function disabled) |
1 |  | display duration of call |
2 |  | display number if metering pulses |
3 (default) |  | display real cost in local currency |

Valid data

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: PD6 © Ericsson Enterprise 2003