BusinessPhone Communication Platform 5.1
Commands > Commands 2000...2999

## 2027
Length of inactivity tone

If you do not dial fast enough (within 8 seconds), the call will be disconnected and you will hear a tone message (TONE.INACT). The duration of this tone is determined by this command.

The time is programmable because of different market requirements Note that this time is used at normal dialling only. If you are disconnected by a service (e.g. information), the time that has been specified by the service will be used, normally 8 seconds.

Value: 1-255 seconds

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2003