BusinessPhone Communication Platform 5.1
Commands > Commands 2000...2999

## 2343
Traffic check at break-in

This command states how the traffic group check should be executed at intrusion.

Alternatives:

0 = It is only necessary that the intruding party is open to call the busy extension. |  |

1 = The intruding party is open to call the busy extension and must also be open to call or receive call from the third party. |  |

2 = The traffic group has to be open in both directions between all parties before the intrusion is allowed. |  |

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2003