BusinessPhone Communication Platform 5.1
Commands > Commands 8000...8999

## 8401
Internal access code

This command defines the internal access code.

This command is only used for Least Cost Routing.

The internal access code (up to 4 digits) is the directory number of a route or trunk to be used to set up calls to the carrier.

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: PD1 © Ericsson Enterprise 2003