BusinessPhone Communication Platform 5.1
Dialogs

## Networking

In this dialog, you can define the general network settings and the settings for network call backs.

To access the dialog, open the “Facilities” menu in the Configuration directory tree and click on “Networking”.

### General

2071 |  | ISID of external voice mailbox

2072 |  | MD110 release version of CN

2073 |  | Removed digits for composing A or B number

2074 |  | Local private code for composing A or B number

2077 |  | 1st central answering position

2078 |  | 2nd central answering position

2079 |  | 3rd central answering position

2084 |  | Type of network call handling

2085 |  | PBX protocol identifier

2087 |  | Transit counter

For more information about a field or a setting, click on the command link in brackets.

### Network Call back

9001 |  | Call setup version at Network CBack

9002 |  | Active time for 'CBack on busy' initPBX

9003 |  | Active time for 'CBack on free' initPBX

9004 |  | Active time for 'CBack on busy' superPBX

9005 |  | Active time for 'CBack on free' superPBX

9006 |  | Maxringtime at the init extension for CBack calls

For more information about a field or a setting, click on the command link in brackets.

#### Actions

Submit |  | To submit your changes to the system. |
Reload |  | To reload the current system settings. |

See Facility Descriptions:

- Networking – Based On Analogue Lines
  (361/15534-ASB 150 02 Uen).
- Networking – VPN Service From PSTN
  (364/15534-ASB 150 02 Uen).
- Networking – Based On Digital Lines
  (365/15534-ASB 150 02 Uen).

Revision: B © Ericsson Enterprise 2003