BusinessPhone Communication Platform 5.1
Commands > Commands 2000...2999

## 2108
MFE time 1

States the supervision time 1 during MFE-signalling.

Supervises the reception of the signals below.

At MFE1 (MFE 2/5) signalling:

- Call class request (A3)
- Group A request (A1)
- All digits request (A6)

At MFE2 (MFE 2/6) signalling:

- Call class request (A3)
- A-number request (A12)
- All digits request (A13)

For other signals, see command 2109 MFE time 2 MFE TIME 2.

Valid values 5-20.

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2003