BusinessPhone Communication Platform 5.1
Commands > Commands 0000...0999

## 0190
Switch to non-IP network allowed ?

The command defines whether or not an extension is allowed to initiate a 'Switch over' of an ongoing call from the IP network to a circuit switched network.

##### Valid data: Yes (default) /No

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: PD6 © Ericsson Enterprise 2003