BusinessPhone Communication Platform 5.1
Commands > Commands 3000...3999

## 3705
ACD-I/O monitor frequence

It is possible to obtain a graphic representation of current traffic to ACD- groups by connecting a PC with a special program, “ACD SUPERVISOR SW PACKAGE”.

The PC is connected to a free V.24 port on EXU or CMU that is stated via command 3706 ACD-I/O port for PC-graph. This command is used to state the interval between the update messages sent to the PC-program.

Range of values: 0-9 in multiples of 4 second intervals |  |

Range of values: 0 means no messages will be sent |  |

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: PD4 © Ericsson Enterprise 2003