BusinessPhone Communication Platform 5.1
Warning Messages ASB 150 02 >

## 0x66
CIL IO Error Channel 0

Default definition: |  | ALARM + INFO + EXTERN + ACTIVE |
Used by block: |  | CL |
Category: |  | MAINTENANCE |

Some error or timeout in the IO handling, detected by the CIL programs for channel number 0.

- D1:
- D2:
- D3: Undefined
- D4: Undefined

#### Recommended action

Verify the connection of the external (peripheral) equipment and the programming of the relevant IO-channel.

Revision: PH2 © Ericsson Enterprise 2003