BusinessPhone Communication Platform 5.1
Dialogs

## Message to CPU

You can send messages to a card in the connected system. The messages are entered as hex-bytes. Only fields that contain data are sent. The message length is adjusted automatically. Up to 20 bytes from any answer that is received is displayed after the execution.

Note

This dialog is only available in online mode!

#### Actions

Submit |  | To submit your changes to the system. |
Clear data fields |  | To clear all data fields except the “ST”, “SN”, “Card” and the “Ind” field. |

See System Description (1551-ASB 150 02 Uen).

Revision: B © Ericsson Enterprise 2003