BusinessPhone Communication Platform 5.1
Commands > Commands 1000...1999

## 1002
Traffic group

The command states to which traffic group the trunk belongs.

The traffic group determines to which trunks and extensions the trunk can be connected.

Trunks (and extensions) can be divided into 16 different traffic groups:

0 = Completely open

1-15 = Checks according to the traffic group matrix

The traffic group matrix specifies which traffic groups are permitted to be connected to each other. It is possible to open one traffic direction, e.g. outgoing, and to bar the opposite-incoming-direction.

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: PD1 © Ericsson Enterprise 2003