BusinessPhone Communication Platform 5.1
Warning Messages ASB 150 02 >

## 0xCA
No Common S-Interface Access Number

Default definition: |  | ERROR |
Used by block: |  | TR |
Category: |  | MAINTENANCE |

A call setup attempt was denied, because of no common number is programmed for the interface.

- D1: Card position
- D2: Individual number
- D3: Undefined
- D4: Undefined

#### Recommended action

Check the programming of the common access number for the ISDN S-interface.

Check command 1956 ‘Common Access Number’.

Revision: PH2 © Ericsson Enterprise 2003