BusinessPhone Communication Platform 5.1
Commands > Commands 4000...4999

## 4503
Predefined info - Text for cordless

With this command the predefined text info strings for cordless instruments are stated. The text string is adapted for 2x12 characters display size and can

contain a maximum of 18 characters.

NOTE! The first 12 characters will be displayed in the first line the last 6 in the second line of cordless display. Rest of string is used for time or date data.

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: PD1 © Ericsson Enterprise 2003