BusinessPhone Communication Platform 5.1
Commands > Commands 2000...2999

## 2621
Special dial tone

The tone indicates that the exchange is ready to accept a digit from the user and that the user has activated a special service, e.g. diversion or programmed information. Compare with dial tone in command 2620 Dial tone.

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2003