BusinessPhone Communication Platform 5.1
Commands > Commands 1000...1999

## 1946
Forced message after timeout

This command states if a CONNECT or ALERTING message shall be sent to network 8 seconds after CALL PROCEEDING. This is to stop timer T303 and force the originating network to through connect the B-channel in order to give the caller the possibility to hear tones or announcements provided by the terminating party. The choice of CONNECT or ALERTING is network dependent.

Valid values: None / Alert / Connect

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: PD1 © Ericsson Enterprise 2003