BusinessPhone Communication Platform 5.1
Warning Messages ASB 150 02 >

## 0xA7
SP Internal Error

Default definition: |  | ERROR |
Used by block: |  | SP |
Category: |  | DESIGNER |

The serial communication processor (SP) on the CPU board has detected an error, that probably is a bug in the SP software.

- D1: Address of error, high byte
- D2: Address of error, low byte
- D3: Undefined
- D4: Undefined

Revision: PH2 © Ericsson Enterprise 2003