BusinessPhone Communication Platform 5.1
Commands > Commands 8000...8999

## 8110
Paging progress time

This command is used to determine the time for the trunk to be connected to the paging equipment to ensure that paging is transmitted.

Range of values = 1-60 s

If the paging equipment sends the acknowledgement signal ‘paging ongoing’ the trunk will be disconnected immediately.

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: PD1 © Ericsson Enterprise 2003