BusinessPhone Communication Platform 5.1
Commands > Commands 8000...8999

## 8035
Guest instrument key F

Depending on type of telephone hotel guests may use a varying number of keys as dial-by-name keys.

DIALOG 2601 |  | has 7 dial-by-name keys. |
DIALOG 3211 |  | has 7 dial-by-name keys. (former DIALOG 3201) |
DIALOG 3212 |  | has 7 dial-by-name keys. (former DIALOG 3202) |
DIALOG 3199 |  | has 1 dial-by-name key. |
DIALOG 3210 |  | has 3 dial-by-name keys. (system release 9 or later) |

The keys are designated A-G in the figures below but are labelled differently on the telephones.

DIALOG 2601: All keys A-G

DIALOG 3211 (3201): All keys A-G
DIALOG 3212 (3202): All keys A-G

DIALOG 3210: Only keys A, E and F

By programming appropriate call numbers for these keys, guests can call various facilities, by a single key pushing, e.g.

- outgoing calls
- reception
- PABX-operator
- service quarter

This command is used to determine to which number calls shall be made when a dial-by-name-key is pressed.

The key function is deactivated by writing over the number with the space character.

The number is common for all guest extensions with DIALOG 2601, DIALOG 3201, DIALOG 3202 or DIALOG 3199 telephones.

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: PD1 © Ericsson Enterprise 2003