BusinessPhone Communication Platform 5.1
Warning Messages ASB 150 02 >

## 0x1D
Data Memory Not Sufficient

Default definition: |  | ALARM + NOPROG + EXTERN + ACTIVE |
Used by block: |  | OS |
Category: |  | MAINTENANCE |

OS could not allocate all requested dynamic memory in the MDATA class. On startup, the operating system allocates data memory depending on the number of program maps mounted on the CPU-board and on the number of boards, used in the system. The memory requirement varies considerably for the different board types available. This warning is sent, if the system finds that the available data memory area is insufficient.

- D1:
- D2: Datamap number

- 00h-0Fh
- FFh: Unmapped memory area

- D3: Undefined
- D4: Undefined

#### Recommended action

The most likely cause of this warning is that the capacity of the system has been exceeded due to the use of too many ELUD type boards. Remove one ELUD type board.

Revision: PH2 © Ericsson Enterprise 2003