BusinessPhone Communication Platform 5.1
Dialogs

## Neighborhood gatekeeper

The gatekeeper gets configured with information about its neighborhood. Symmetry is not required when programming neighborhood gatekeepers (i.e. if the GK1 is configured as neighborhood gatekeeper for GK2, it is not obligatory that the GK2 is programmed as neighborhood gatekeeper for GK1). The following information is configured manually:

- Primary neighborhood gatekeeper RAS transport address
- Primary neighborhood gatekeeper identifier
- Backup neighborhood gatekeeper RAS transport address - optional
- Backup neighborhood gatekeeper identifier - conditionally mandatory
- Alias address(es) for which the neighborhood gatekeeper is responsible

The gatekeeper will keep track of its neighborhood gatekeeper’s status and on the call base decide if the location requests will be sent to the primary or to the backup position.

#### Actions

Submit |  | To submit your changes to the system. |
Back |  | To go back to the previous screen. |
Reload |  | To reload the current system settings. |

See also facility description Networking via Voice over IP Lines (366/155 34-ASB 150 02 Uen)

Revision: B © Ericsson Enterprise 2003