BusinessPhone Communication Platform 5.1
Warning Messages ASB 150 02 >

## 0x22
Message To/From Rp Discarded

Default definition: |  | ERROR |
Used by block: |  | OS |
Category: |  | DESIGNER |

OS has received a message to / from a RP, but the message is not accepted as valid. The message is not passed to the final receiver.

- D1: Card position (sender or receiver)
- D2: Type of error

- Bit 0: Illegal Data Field Discriminator (DFD)
- Bit 1: Illegal message type sequence
- Bit 2: Invalid ID in message
- Bit 3: Invalid part number
- Bit 4: Invalid ML
- Bit 5: Spare
- Bit 6: Illegal IND number
- Bit 7: No OS buffer available

- D3: Undefined
- D4: Undefined

Revision: PH2 © Ericsson Enterprise 2003