BusinessPhone Communication Platform 5.1
Commands > Commands 3000...3999

## 3834
Overflow time in sec for rerouting

This command defines whether the value programmed in command 3825 is interpreted as minutes or as seconds.

##### Valid data

MINUTES |  | (Default) |
SECONDS |  |  |

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: PD4 © Ericsson Enterprise 2003