BusinessPhone Communication Platform 5.1
Signal Types, Internal Messages and CSW-Blocks > Internal Messages - Info Codes > Sorted by Info code

## AD METER

0 METSTART |  | Init metering |
1 METCHANGE |  | Int metering for new extension/trunk |
2 METREL |  | Stops metering |
3 METRDYCHG |  | Metering for a call is ended and restarted |
4 METRDYREL |  | Metering for a call is ended and released |
5 METCONQ |  | Ask for pulses and duration |
6 METANSW |  | Answer |
9 METSEIZ |  | Seizure of a meter |
10 METSEIZACK |  | Answer, metering present and available |
11 METSEIZNAKNA |  | Answer, metering equipment not present |
12 METSEIZNAKB |  | Answer, metering equipment busy |
14 METAOCNAK |  | Reject of metering at ISDN |
15 METREADCALL |  | Answer message for current call |
16 METRESETCALL |  | Reset addressed accumulator of a caller |
17 METACKCALL |  | Answer contained accumulated pulses |
18 METNAKCALL |  | Negative answer to read or reset |
19 METCONANSW |  | Answer message for current call |
20 METLASTCALL |  | Last adding to meter of caller |
21 METSAVECALL |  | Adding to meter of a caller |
22 METLASTTRNK |  | Last adding to meter of a trunk |
23 METSAVETRNK |  | Adding to meter of a trunk |

Revision: PD2 © Ericsson Enterprise 2003