BusinessPhone Communication Platform 5.1
Commands > Commands 1000...1999

## 1011
Reroute on answering position vacant?

The command is used for in-dialing and for private lines to reroute incoming calls to the rerouting position, if the required destination is vacant.

For rerouting to take place, the rerouting position must have been programmed, see commands 1103 Reroute position at day and 1104 Reroute position at night.

Valid values: YES / NO

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: PD1 © Ericsson Enterprise 2003