BusinessPhone Communication Platform 5.1
Signal Types, Internal Messages and CSW-Blocks > Internal Messages - Info Codes > Sorted by Info code

## B5 TISIG

1 TISEIZ |  | RP Call to Cordless |
2 TIRELEASE |  | RP Disconnection in ASB |
3 TICLIP |  | RP Call update to cordless |
4 TIMWI |  | RP Turn on message waiting indication |
5 TIIDLE |  | RP Send idle display information |
6 TIINCALL |  | RP Send in call display information |
7 TICONN |  | RP Send connected information |
8 TIREDIR |  | RP Send redirected information |
32 TIDISC |  | RP Disconnection from the Cordless |
33 TISEIZACK |  | RP Seizure of Cordless accepted |
34 TISEIZNAK |  | RP Seizure of Cordless rejected |
35 TIALERT |  | RP Cordless has started ringing |

Revision: PD2 © Ericsson Enterprise 2003