BusinessPhone Communication Platform 5.1
Commands > Commands 4000...4999

## 4007
Queue announcement reference

A voice message can be supplied to external incoming calls in the PBX-operator queue. This command is used to state the reference number for a voice message.

The reference number is entered as: uuvv

where

uu = 01 (always) |  |

vv = 01-32 (see command 4401 Voice Announcements) |  |

uuvv = blank (no voice message) |  |

It is required that the stated reference (uuvv) has been recorded with a system telephone in accordance with command 4401 Voice Announcements.

The duration of the voice message shall be stated with command 4006 Queue announcement time.

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: PD1 © Ericsson Enterprise 2003