BusinessPhone Communication Platform 5.1
Facility Description – General

## Display Messages

Telephones with display supplies information concerning name, directory number and status of call partner.

The display is also used when programming individual or system related functions.

Display information show some difference between the various telephones that may be connected.

Below is an overview of the display types.

### EXECUTIVE Telephone, DBC 213

This telephone has 3 rows:

Row 1 shows the date and time and eventually the temperature.

Row 2 shows the connected party

The bottom row shows the 4 menu functions that are activated by the 4 keys below.

### STANDARD Telephone, DBC 212 and DBC 631

The display has two rows:

Row 1 shows date and time. It is also used for displaying the diverted party in a call.

Row 2 shows called/calling/connected party.

### EXECUTIVE Telephone, DBC 662

Row 1 shows always date, time and temperature.

Row 2 is reserved for ACD-queue information when the telephone is used as an ACD-agent position.

Row 3 shows information only if the called or calling party is diverted.

Row 4 shows the calling or connected party

If the Menu key is pressed the display show a menu on row 4. The menu options can be activated by the four menu keys below the display.

### EXECUTIVE Telephone, DBC 753

The upper row shows information only when the call is diverted.

The lower row shows the calling or connected party.

If the Menu key is pressed the display show a menu on row 2. The menu options can be activated by the four menu keys below the display.

### OPERATOR’s Console, DBC 214

This telephone has 5 rows:

Top row shows the date and time and eventually the temperature.

Second row shows the indication of the Common and Individual operator queue.

The 3rd and 4th row show the connected party.

The bottom row shows the 4 menu functions that are activated by the 4 keys below.

### OPERATOR’s Console, DBC 663 and DBC 754

On the OPERATOR’s Console the area is used for programming with the same display picture as for the 2*20 character display.

Revision: PC1 © Ericsson Enterprise 2003